QAPlus/Info V5.01 
for MediaVision
Copyright (c) 1989-1992  DiagSoft, Inc.
All Rights Reserved
IRQ/DMA detection
System Software:        Interrupt Assignments
ROM BIOS: Award         IRQ 00: Timer 
DOS Version: 5.00       IRQ 01: Keyboard 
                        IRQ 02: [CASCADE] 
DMA Channel Usage:      IRQ 03: COM2 
DMA 0: Available *      IRQ 04: COM1 
DMA 1: Available *      IRQ 05: Available *
DMA 2: Floppy           IRQ 06: Floppy 
DMA 3: Available *      IRQ 07: Available *
DMA 4: [CASCADE]        IRQ 08: Clock/Cal 
DMA 5: Available *      IRQ 09: OCCUPIED 
DMA 6: Available *      IRQ 10: Available *
DMA 7: Available *      IRQ 11: Available *
                        IRQ 12: OCCUPIED 
                        IRQ 13: NPU 
                        IRQ 14: OCCUPIED 
* Not used by any       IRQ 15: Available *
  standard device       no IRQ: LPT1 
Hardware Configuration
Processor Type ....... 80486
Numeric Processor .... 80486DX
Base Memory Size ..... 637K
Ext Memory ........... 4608K
Ext Memory Available . 0K
Exp Memory ........... 1024K
Exp Memory Available . 1024K
Primary Video ........ VGA
  Video BIOS ......... Quadtel
  Text Base Address .. B800h
Secondary Video ...... None
Video mode, EGA switch 03h, sw(1-4) 1001
DOS Hard Drives ...... C:[503M] 
Clock Type ........... AT
COM Ports ............ COM1[03F8h] COM2[02F8h] 
LPT Ports ............ LPT1[0378h] 
Mouse Driver ......... none
Game Ports ........... none
