ROManager for the MegaFlash - ATTENTION: This shortcut does not replace the handbook -RMA.TXT on Disc!!! Please read it!!!
--------------------------- - ========== ---------------------------------------------------------------------------------
Files (Programs)
----- ----------
- MegaFlashROManager_FutureOS_V1.46.dsk ..... - contain the -MegaFlash- versions of ROManager for FutureOS

- MegaFlashROManager_4_BASIC_V1.45_ROM&Booster.DSK ..... - contains the 16 KB ROMs for the ROM Version 1.45 for MegaFlash

- MegaFlashROManager_4_BASIC_V1.45.dsk ..... - contains the -MegaFlash- versions of ROManager for CPC-OS Ver. 1.45

- MegaFlashGordonROManager_4_BASIC_V1.45.dsk - contains the FlashGordon versions of ROManager for CPC-OS Ver. 1.45

- 464 MegaFlashROManager_FG_BASIC_V1.45 2013-03-06.dsk ..... - contains 64 KB versions for CPC464/664 and MegaFlash

Files (Sources)
----- ---------
- 180 MegaFlashROManager_FutureOS_V1.46 2014-02-20.dsk - contains the FG Source Code of the ROManager for FutureOS 1.46

- AAA MegaFlashROManager_BASIC_V1.47 2013-03-19.dsk - contains the Source Code for the FlashGordon MegaFlash device.

Additional files (ROMs)
=======================
For the MegaFlash device:
-------------------------
- -RMA----.ROM: ROManager, start with !RMA
- -RMA---B.ROM: ROManager and the Booster to enable all 32 ROMs. Locate this ROM at position 15!
- -RMA-L--.ROM: ROManager, it will ask you for your preferred language.
- -RMA-L-B.ROM: ROManager and the Booster to enable all 32 ROMs. It will ask you for your preferred language. Place at 15!

The folder ROMs contains the following files:
---------------------------------------------
- 900 CPC_ROMs_16KB_I.dsk -- A Vortex disc full with cool application ROMs (use SF2 ROManager_FutureOS to install them)
- 900 CPC_ROMs_16KB_I.txt -- Inventory of the ROMs on disc I
- 900 CPC_ROMs_16KB_II.dsk - Another Vortex disc full with cool GAME- and application ROMs (use SF2 ROManager_FutureOS)
- 900 CPC_ROMs_16KB_II.txt - Inventory of the ROMs on disc II

How to start ROManager for FutureOS? Only this version can use the EDIT ROM function!
------------------------------------
- Insert Disc in Drive A (or B)
- Start FutureOS with |OS
- Tag drive A (or B). That means click at the drive Icon that contains the Disc with ROManager
- Click at the DIR Icon
- Tag the first file on the Disc ("- ROManager")
- Now click the RUN Icon

How to start ROManager for BASIC?
---------------------------------
- Insert Disc in Drive A (or B)
- Select drive with |A (or |B). That means select the drive that contains the Disc with ROManager
- Type CAT (then press ENTER) for the CATalog, now you see the files
- Type RUN"-RMA.BAS", then Enter

How to start ROManager from ROM?
--------------------------------
- Type the RSX command |RMA, and then ENTER

Beware: If using a ROManager ROM with included Booster then this ROM MUST be placed at ROM select / ROM number 15!

How to install the ROManager ROM?
---------------------------------
- Read the documentation on disc, the file has the name "-RMA.TXT"
- Use the Disc version of ROManager to install one of the ROM files "-RMA-?-?.ROM". Where L=Language and B=Booster.
  (-RMA-L-B.ROM for example contains the ROManager and the ROM Booster, it asks you for your language)
  If you choose the version with the Booster (ROM -RMA---B.ROM or -RMA-L-B.ROM), then you have to install it at 
  ROM position 15!!! The Booster allows using all 32 ROMs of the MegaFlash.
- Reset the CPC
- You can use the ROManager ROM now by typing the RSX command "|RMA" in small or upper letters

How to use ROManager on a CPC464 or CPC664 with only 64 KB RAM?
---------------------------------------------------------------
- Start file "-RMA.BAS" on DSK image: 464 MegaFlashROManager_BASIC_V1.45 2013-02-20.dsk
- Enter number 1-5 for language, press Enter or Return
- Use the program like told in the little handbook, it's name is "-RMA.TXT"


Enjoy your MegaFlash and the ROManager,
TFM of FutureSoft - 2014.03.28
