ROManager for the SYMBiFACE II - ATTENTION: This shortcut does not replace the handbook -ROM.TXT on Disc!!! Please read it!
------------------------------ - ========== -------------------------------------------------------------------------------
Files (Programs)
----- ----------
- SF2 ROManager_FutureOS V1.46.dsk .......... - contain the Disc versions of the SF2 ROManager for FutureOS
- SF2 ROManager_4_BASIC_V1.45_ROM&Booster.dsk - contains the ROM version of the SF2 ROManager, with/without the ROM Booster
- SF2 ROManager_4_BASIC_V1.45.dsk ........... - contain the Disc versions of the SF2 ROManager for BASIC

Files (Sources)
----- ---------
- 180 SF2 ROManager V1.46 FutureOS 2014-02-20.dsk - contain the Source Code of the SF2 ROManager for FutureOS
- AAA SF2 ROManager V1.45_BASIC_2013-04-19.dsk .. - contains the Source Code of the SF2 ROManager for the CPC-OS

Additional files:
-----------------
The folder ROMs contains the following files:
- 900 CPC_ROMs_16KB_I.dsk -- A Vortex disc full with cool application ROMs (use SF2 ROManager_FutureOS to install them)
- 900 CPC_ROMs_16KB_I.txt -- Inventory of the ROMs on disc I
- 900 CPC_ROMs_16KB_II.dsk - Another Vortex disc full with cool GAME- and application ROMs (use SF2 ROManager_FutureOS)
- 900 CPC_ROMs_16KB_II.txt - Inventory of the ROMs on disc II

How to start ROManager for FutureOS? ATTENTION: Only the FutureOS version can use the EDIT ROM function
------------------------------------
- Insert Disc in Drive A (or B)
- Start FutureOS with |OS
- Tag drive A (or B). That means click at the drive Icon that contains the Disc with ROManager
- Click at the DIR Icon
- Tag the first file on the Disc ("- ROManager")
- Now click the RUN Icon

How to start ROManager for BASIC?
---------------------------------
- Insert Disc in Drive A (or B)
- Select drive with |A (or |B). That means select the drive that contains the Disc with ROManager
- Type CAT (then press ENTER) for the CATalog, now you see the files
- Type RUN"-RMA.BAS", then Enter

How to start ROManager from ROM?
--------------------------------
- Type the RSX command |RMA, then ENTER

How to install the ROManager ROMs?
----------------------------------
- Read the documentation on disc, the file has the name "-RMA.TXT"
- Use the Disc version of ROManager to install the ROM file "SF2RMA.ROM" (just the ROManager) or the ROM file "SF2RMABO.ROM"
  (contains the ROManager and the ROM Booster) into an empty ROM position. If you choose the version with the Booster, then
  you have to install it at ROM position 15. The Booster allows using all 32 ROMs of the SYMBiFACE II.
- Reset the CPC
- You can use the ROManager ROM now by typing the RSX command "|RMA" in small or upper letters.


Have fun,
TFM
